|  |  |
| --- | --- |
| FPGA device selected: | xc6slx100 |
| Total Number of occupied Slices: | 15822 |
| Total Number of Slice Flip Flops: | 126576 |
| Total Number of Slice LUTs: | 63288 |
| Cortex-M0 Number of occupied Slices: | 1131 |
| Cortex-M0 Number of Slice Flip Flops: | 872 |
| Cortex-M0 Number of Slice LUTs: | 3156 |
| Bridge Number of occupied Slices: | 7 |
| Bridge Number of Slice Flip Flops: | 4 |
| Bridge Number of Slice LUTs: | 5 |
| Best possible clock frequency: | 77.863MHz |